**Prosedyre – arbeid med kreftfremkallende og mistenkt kreftfremkallende stoffer**

Med kreftfremkallende stoffer menes stoffer med faresetningene H350, H350i og H351

* Arbeid med kreftfremkallende stoffer skal risikovurderes grundig
* Alt arbeid med slike stoffer, også veiing, skal utføres i avtrekksskap, veiekabinett eller annen forsvarlig ventilasjon dersom det er risiko for damp eller støv
* Kreftfremkallende stoffer skal alltid oppbevares og transporteres i tydelig merket, lukket emballasje
* Alt arbeid med kreftfremkallende stoffer skal registreres i bedriftens eksponeringsregister og arbeidstaker delta på helseundersøkelse hos bedriftshelsetjenesten
* Redskaper skal rengjøres i avtrekksskap og vaskevann/løsningsmidler skal samles opp og avhendes som farlig avfall
* Arbeidssted skal rengjøres grundig etter arbeid. Engangsklut/fuktet papir skal benyttes, samles opp i egnet beholder og avhendes som farlig avfall
* Avfall skal legges i særskilte avfallsbeholdere
* Ved endt arbeid skal man vaske hendene
* Arbeidsklær:
	+ Ved arbeid med kreftfremkallende stoffer skal labfrakk, vernebriller og egnede hansker benyttes
	+ Ved søl skal hansker vrenges og labfrakk samles i egnet beholder og avhendes som farlig avfall
	+ Labfrakk skal oppbevares på lab
* Gravide og ammende kvinner skal ikke arbeide med kreftfremkallende stoffer
* Kreftfremkallende kjemikalier skal oppbevares i låst kjemikalieskap

Kilder:

<https://www.arbeidstilsynet.no/tema/kjemikalier/laboratoriearbeid/>

<https://www.arbeidstilsynet.no/regelverk/forskrifter/forskrift-om-utforelse-av-arbeid/2/3/3-11/>

<https://innsida.ntnu.no/wiki/-/wiki/Norsk/Eksponeringsregister>

**Procedure – working with carcinogenic and suspected carcinogenic substances**

By carcinogenic substances we mean substances marked with hazard statements H350, H350i and H351.

* Work with carcinogenic substances has to be thoroughly risk assessed
* All work with such substances, including weighing, has to be performed in a fume hood, weighing cabinet or use other properly ventilated systems/equipment if there’s a risk of evaporation or dust
* Carcinogenic substances must be stored and transported in clearly labeled, closed containers
* All work with carcinogenic substances must be registered in the exposure index of the company and employees should participate in a health check-up at the company health service
* Equipment has to be thoroughly cleaned inside the fume hood and waste water/solvents must be collected and disposed of as hazardous waste
* The work place must be thoroughly cleaned when the experiment is done. Use a disposable wash cloth or moist paper which is collected in an appropriate container and disposed as hazardous waste
* Excess chemicals and/or chemical waste must be collected in special containers
* Remember to wash your hands when the experiment is done
* Work clothes:
	+ When working with carcinogenic substances, always use a lab coat, safety glasses and suitable gloves
	+ The lab coat should always be kept in the lab
	+ After a spill, turn the gloves inside out, collect your lab coat in an appropriate container and dispose as hazardous waste
* Pregnant and breastfeeding women shall not work with carcinogenic substances
* Carcinogenic substances have to be stored in a locked chemical cabinet